Switch 2

ena

conf

hostname SW2

banner motd #

SW2 duoc cau hinh boi HungKQ#

enable password 123

line console 0

password 123

login

exit

line vty 0 15

password 123

login

exit

service password-encryption

interface vlan 1

ip address 100.8.5.2 255.255.255.0

no shutdown

exit

ip default-gateway 100.8.5.1

exit

copy running-config startup-config

Switch 1

ena

conf

hostname SW1

banner motd #

SW1 duoc cau hinh boi HungKQ#

enable password 123

line console 0

password 123

login

exit

line vty 0 15

password 123

login

exit

service password-encryption

interface vlan 1

ip address 192.0.9.2 255.255.255.0

no shutdown

exit

ip default-gateway 192.0.9.1

exit

copy running-config startup-config

Router

enable

configure

enable password 123

line console 0

password 123

login

exit

line vty 0 15

password 123

login

exit

service password-encryption

banner motd #R1 duoc cau hinh boi Hung#

hostname R1

exit

copy running-config startup-config

SW1#copy

SW1#copy sta

SW1#copy startup-config t

SW1#copy startup-config tftp:

Address or name of remote host []? 192.0.9.6