An internal switch setting that controls whether an interrupt can be processed or not. The mask is a bit that is turned on and off by the program.